# Warning signal for unauthorised person

## Description:

[**Automation, security feature Unauthorised Door Open Detection - Securing doors against the unauthorized door opening in 2N® IP Intercom.**](https://faq.2n.cz/pages/viewpage.action?pageId=76808795)

This automation will cause a sound to be played once the door is open without authorization.

A close up of a map

Description automatically generated

# Intercom Door Configuration:

If you have previously configured the unauthorized door open setting please follow the steps below.

1. Unauthorized Open Door. Once an unauthorized open door is detected, a signal is sent to play a user sound.
2. Play User Sound. The sound played when the door is opened without authorization.

1: Upon login select the Hardware option.

A close up of a logo

Description automatically generated

2: From the left-hand menu select Door.

A screenshot of a cell phone

Description automatically generated

3: In the Door tab, enable the Unauthorized Door open Detection. As well, set the Door Sensor to the correct Input and then save the settings.

A screenshot of a cell phone

Description automatically generated

Date of automation design: 07/17/2020

Firmware Version: 2.29.1.38.8

List of compatible Hardware:

* 2N IP Verso
* 2N IP Vario
* 2N IP Force
* 2N IP Safety
* 2N IP Base
* 2N IP Solo
* 2N LTE Verso

List of automation parameters:

* Sound
* Destination
* Channel

Requirements:

* 2N Intercom
* 2N Enhanced Integration Licence (or Gold Licence) \*Not applicable to the USA
* Door Sensor